; Printer data section description.
;
; UpdateName        == .ini type profile,
;                      .ini config sect,
;                      default,
;                      .ini sect flag,
;                      multiple config flag
;
; Where:
;
; UpdateName        == Name of printer description section within this file.
;                      In WIN.INI, when [device] is the section name,
;                      UpdateName is the keyname.  This is where setup
;                      looks to map a "printer=4" keyname from WIN.INI.
;
; .ini type profile == This is the profile string setup uses to find the
;                      printer description index from the printer 
;                      configuration information section in the
;                      Win 3.0 WIN.INI.  (When the ".ini config sect"
;                      is the section name, this is the keyname in WIN.INI).
;
; .ini config sect  == This is the name of the Win 3.0 win.ini printer 
;                      configuration section for the printer (minus the port
;                      config info).
;
; default           == This is the default profile used to obtain a printer 
;                      description string from this file if we are unable to
;                      get a description profile from the Win 3.0 win.ini.
;                      This is for the "unconfigured printer case".
;
; .ini sect flag    == This tells setup whether or not to use port 
;                      configuration info to create the Win 3.0 win.ini
;                      printer configuration section name.  For example:
;                      The HPPCL section name look like [HPPCL,port], while
;                      the EPSON configuration section always looks like 
;                      [epson9drv], lacking any port information. Set this 
;                      flag to 1 if the win.ini config section does NOT use 
;                      port information to create the section name. Leave the 
;                      field NULL if port information should be used.
;
; multiple config flag == This flag is set 1 if only a single printer can be 
;                         configured for the driver. Leave the flag NULL if
;                         the driver can setup multiple configuration 
;                         sections.
;
;For single model drivers, the paper orientation is used
;to force setup to use the given modelname string.
[Printer.Data]
"Canon BJ-10v/300J/330J"    = "model",        "Canon BJ-10v/300J/330J", "BJ-10v",1,1
"Canon LBP-B406S/D"         = "printer",      "Canon LBP-B406S/D,",     1
"EPSON (ESC/P)"             = "Printer Name", "EPSON (ESC/P)",          "AP300",1,1
"EPSON (ESC/Page)"          = "Model",        "EPSON (ESC/Page)",       7,1,1
"EPSON LP-7000/3000"        = "Model",        "EPSON LP-7000",          7,1,1
"EPSON (ESC/Page Bitmap)"   = "Model",        "EPSON (ESC/Page Bitmap)",7,1,1
"HP DeskJet J-Series v1.0"  = "prtindex",     "DJ505J,",                0
"NEC NM"                    = "Model",        "NEC NM",                 NM2010,1,1
"NEC NPDL"                  = "Model",        "NEC NPDL",               PR2000,1,1
"NPDL Level2 Printer"       = "device",       "NPDL2,",                 2
"NEC PC-PR101/T PRINTER"    = "Prn",          "NEC PC-PR101/T PRINTER", 135,1,1
"NEC PC-PR150V PRINTER"     = "Prn",          "NEC PC-PR150V PRINTER",  138,1,1
"NEC PC-PR201"              = "Printer Model","NEC PC-PR201",           PR201H,1,1
"NEC PC-PR602"              = "Model",        "NEC PC-PR602",           PR602R,1,1
"EPSON PostScript"          = "device",       "PostScript,",            "EPSON LP-3000PS F2"
"OKI PostScript 78"         = "device",       "PostScript,",            1
"OKI PostScript 83"         = "device",       "PostScript,",            1
"RICOH PC LASER"            = "Model",        "RICOH PC LASER",         "SP4mk2",1,1

[Canon BJ-10v/300J/330J]
BJ-10v        = "Canon Bubble-Jet BJ-10v"
BJ-10v/Custom = "Canon Bubble-Jet BJ-10v Custom"
BJ-10v Select = "Canon Bubble-Jet BJ-10v Select"
BJ-15v        = "Canon Bubble-Jet BJ-15v"
BJ-300J       = "Canon Bubble-Jet BJ-300J"
BJ-330J       = "Canon Bubble-Jet BJ-330J"

[Canon LBP-B406S/D]
1 = "Canon LBP-B406S LIPS3"
2 = "Canon LBP-B406D LIPS3"
3 = "Canon LBP-A404 LIPS3"
4 = "Canon LBP-B406E LIPS3"
5 = "Canon LBP-A404E LIPS3"
6 = "Canon LBP-A304E LIPS3"
7 = "Canon LBP-B406G LIPS3"

[EPSON (ESC/P)]
AP1000  = "EPSON AP-1000"
AP300   = "EPSON AP-300"
AP500   = "EPSON AP-500"
AP800   = "EPSON AP-800"
AP900   = "EPSON AP-900"
FBP3000 = "EPSON FBP-3000"
HG2000  = "EPSON HG-2000"
HG4000  = "EPSON HG-4000"
HG5130  = "EPSON HG-5130"
HG800   = "EPSON HG-800"
VP1000  = "EPSON VP-1000"
VP1500  = "EPSON VP-1500"
VP2000  = "EPSON VP-2000"
VP2600  = "EPSON VP-2600"
VP300   = "EPSON VP-300"
VP4800  = "EPSON VP-4800"
VP800   = "EPSON VP-800"
VP900   = "EPSON VP-900"
XP2000  = "EPSON XP-2000"

[EPSON (ESC/Page)]
2 = "EPSON LP-2000"
3 = "EPSON LP-3000"
7 = "EPSON LP-7000/7000G"
8 = "EPSON LP-8000"

[EPSON LP-7000/3000]
2 = "EPSON LP-2000"
3 = "EPSON LP-3000"
7 = "EPSON LP-7000/7000G"
8 = "EPSON LP-8000"

[EPSON (ESC/Page Bitmap)]
2 = "EPSON LP-2000"
3 = "EPSON LP-3000"
7 = "EPSON LP-7000/7000G"
8 = "EPSON LP-8000"

[HP DeskJet J-Series v1.0]
; Windows 3.1 HP DeskJet 505J driver not support Color
; 0 = "HP DeskJet 505J"
1 = "HP DeskJet 500J"

[EPSON PostScript]
"EPSON LP-3000PS F2" = "EPSON LP-3000PS F2"
"EPSON LP-3000PS F5" = "EPSON LP-3000PS F5"

[OKI PostScript 78]
1 = "OKI MICROLINE 801PS"
2 = "OKI MICROLINE 801PS+F"
3 = "OKI OPP6008PS"
"OKI ML801PS"                = "OKI MICROLINE 801PS"
"OKI ML801PS (Kanji)"         = "OKI MICROLINE 801PS"
"OKI ML801PS (Kanji 2 Typefaces)"   = "OKI MICROLINE 801PS"
"OKI ML801PS+F"              = "OKI MICROLINE 801PS+F"
"OKI ML801PS+F (Kanji)"       = "OKI MICROLINE 801PS+F"
"OKI ML801PS+F (Kanji 5 Typefaces)" = "OKI MICROLINE 801PS+F"
"OKI OPP6008PS"              = "OKI OPP6008PS"
"OKI OPP6008PS (Kanji)"       = "OKI OPP6008PS"
"OKI OPP6008PS (Kanji 2 Typefaces)" = "OKI OPP6008PS"

[OKI PostScript 83]
1 = "OKI MICROLINE 801PS"
2 = "OKI MICROLINE 801PS+F"
3 = "OKI OPP6008PS"
"OKI ML801PS"                = "OKI MICROLINE 801PS"
"OKI ML801PS (Kanji)"         = "OKI MICROLINE 801PS"
"OKI ML801PS (Kanji 2 Typefaces)"   = "OKI MICROLINE 801PS"
"OKI ML801PS+F"              = "OKI MICROLINE 801PS+F"
"OKI ML801PS+F (Kanji)"       = "OKI MICROLINE 801PS+F"
"OKI ML801PS+F (Kanji 5 Typefaces)" = "OKI MICROLINE 801PS+F"
"OKI OPP6008PS"              = "OKI OPP6008PS"
"OKI OPP6008PS (Kanji)"       = "OKI OPP6008PS"
"OKI OPP6008PS (Kanji 2 Typefaces)" = "OKI OPP6008PS"

[NEC NM]
NM2010 = "NEC NM-2010"
NM4150 = "NEC NM-4150"
NM9950 = "NEC NM-9950/9950II"
NM5020 = "NEC NM-5020/5020L"
NM9700 = "NEC NM-9700"
NM9900 = "NEC NM-9900"

[NEC NPDL]
PR601  = "NEC PC-PR601"
PR602  = "NEC PC-PR602"
PR602R = "NEC PC-PR602R"
PR1000 = "NEC PC-PR1000"
PR2000 = "NEC PC-PR2000"

[NPDL Level2 Printer]
1 = "NEC PC-PR1000/4"
2 = "NEC PC-PR2000/2"
3 = "NEC PC-PR2000/4"
4 = "NEC PC-PR4000/4"
5 = "NEC PC-PR4000E/4"

[NEC PC-PR101/T PRINTER]
135 = "NEC PC-PR201/TC100"
138 = "NEC PC-PR101/T67"

[NEC PC-PR150V PRINTER]
135 = "NEC PC-PR350"
137 = "NEC PC-PR150VH"
138 = "NEC PC-PR150V"
139 = "NEC PC-PR150T"
146 = "NEC PC-PR150N"

[NEC PC-PR201]
PR201L = "NEC PC-PR201"
PR201M = "NEC PC-PR201"
PR201H = "NEC PC-PR201"
PR101L = "NEC PC-PR101"
PR101  = "NEC PC-PR101"

[NEC PC-PR602]
PR601  = "NEC PC-PR601"
PR602  = "NEC PC-PR602"
PR602R = "NEC PC-PR602R"
PR1000 = "NEC PC-PR1000"
PR2000 = "NEC PC-PR2000"

[RICOH PC LASER]
SP4    = "RICOH PC-LASER SP4mkII"
SP4mk2 = "RICOH PC-LASER SP4mkII"
SP5    = "RICOH PC-LASER SP5"

;
; This section facilitates the translation of printer description
; strings pulled from .WPD files into "true printer names". We do
; this so that these printers will be properly upgraded since the
; WPD printer names may not match the printer names listed in
; control.inf.
;
; "WPD description prefix",    "True printer name"
;
; The code will attempt to match the WPD desciption aginst the N chars
; of each of the first fields below. If a match is found, the code
; utilizes the description in field 2 and the printer name.
;
[WPD_NickNames]
"Apple LaserWriter II NTX-J",  "Apple LaserWriter II NTX-J"
"Canon LBP-A404PS Lite",       "Canon LBP-A404PS Lite"
"Canon LBP-A404PS",            "Canon LBP-A404PS"
"EPSON LP-3000PS F2",          "EPSON LP-3000PS F2"
"EPSON LP-3000PS F5",          "EPSON LP-3000PS F5"
"Fujitsu FMLBP211PS",          "Fujitsu FMLBP211PS"
"NEC PC-PR3000PS/4F 400dpi",   "NEC PC-PR3000PS/4F 400dpi"
"NEC PC-PR3000PS/4 400dpi",    "NEC PC-PR3000PS/4 400dpi"
"NEC PC-PR3000PS 320dpi",      "NEC PC-PR3000PS 320dpi"
"NEC PC-PR602PS 320dpi",       "NEC PC-PR602PS 320dpi"
"NEC PC-PR800PS/3",            "NEC PC-PR800PS/3"
"OKI MICROLINE 801PS+F",       "OKI MICROLINE 801PS+F"
"OKI MICROLINE 801PS",         "OKI MICROLINE 801PS"
"OKI OPP6008PS",               "OKI OPP6008PS"
